

AssetLink Iridium Device Configuration Guide

*March 2019*

**AssetLink Global LLC**

[**www.assetlinkglobal.com**](http://www.assetlinkglobal.com/)

[**service@assetlinkglobal.com**](mailto:service@assetlinkglobal.com)

**+1 (303) 862.8745**

**Fax: +1 (720) 862.3515**

**Revision History**

|  |  |  |
| --- | --- | --- |
| **Revision** | **Date of Release** | **Purpose** |
| Initial Draft | 3/1/2019 | Iridium device configuration guide for customers setting up devices on their own Iridium account. |

**Introduction**

The purpose of this documentation is to provide AssetLink customers direction in setting up AssetPack devices on their own Iridium account.

To set up an AssetPack on Iridium, on the SBD->Contract->New page enter the values as follows:

**Destination:** mapdata.assetlinkglobal.com:6699

**Ring Alerts:** “Yes”

**Method:** “Direct IP”

**Include Geo Data:** “Checked”

**MO ACK:** “Checked”

All other values are specific to the AssetLink customer’s Iridium account.

Once the AssetPack is set up on Iridium and turned on in a location it can see the sky, it will start reporting and data will flow into the AssetLink Device Manager.  The reporting schedule for the device will be as per the schedule it was programed with prior to shipment.

Example AssetPack configuration on the Iridium SBD->Contract->New page.

